(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 21)
    (zones 0)
    (modules 8)
    (nets 41)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 Gnd)
  (net 2 "Net-(K1-Pad3)")
  (net 3 Compressor_Power)
  (net 4 Compressor_Signal)
  (net 5 120VAC)
  (net 6 "Net-(K2-Pad3)")
  (net 7 "Net-(K3-Pad2)")
  (net 8 "Net-(K3-Pad3)")
  (net 9 "Net-(K3-Pad4)")
  (net 10 "Net-(K3-Pad5)")
  (net 11 "Net-(K3-Pad1)")
  (net 12 "Net-(K4-Pad1)")
  (net 13 "Net-(K4-Pad5)")
  (net 14 "Net-(K4-Pad4)")
  (net 15 "Net-(K4-Pad3)")
  (net 16 "Net-(K4-Pad2)")
  (net 17 "Net-(K5-Pad2)")
  (net 18 "Net-(K5-Pad3)")
  (net 19 "Net-(K5-Pad4)")
  (net 20 "Net-(K5-Pad5)")
  (net 21 "Net-(K5-Pad1)")
  (net 22 "Net-(K6-Pad1)")
  (net 23 "Net-(K6-Pad5)")
  (net 24 "Net-(K6-Pad4)")
  (net 25 "Net-(K6-Pad3)")
  (net 26 "Net-(K6-Pad2)")
  (net 27 "Net-(U1-Pad9)")
  (net 28 "Net-(U1-Pad10)")
  (net 29 "Net-(U1-Pad11)")
  (net 30 "Net-(U1-Pad12)")
  (net 31 "Net-(U1-Pad13)")
  (net 32 "Net-(U1-Pad14)")
  (net 33 "Net-(U1-Pad15)")
  (net 34 "Net-(U1-Pad16)")
  (net 35 5VDC)
  (net 36 "Net-(U1-Pad3)")
  (net 37 OWC_BUS)
  (net 38 "Net-(U1-Pad6)")
  (net 39 "Net-(U1-Pad7)")
  (net 40 "Net-(U1-Pad8)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5VDC)
    (add_net Compressor_Signal)
    (add_net Gnd)
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(K2-Pad3)")
    (add_net "Net-(K3-Pad1)")
    (add_net "Net-(K3-Pad2)")
    (add_net "Net-(K3-Pad3)")
    (add_net "Net-(K3-Pad4)")
    (add_net "Net-(K3-Pad5)")
    (add_net "Net-(K4-Pad1)")
    (add_net "Net-(K4-Pad2)")
    (add_net "Net-(K4-Pad3)")
    (add_net "Net-(K4-Pad4)")
    (add_net "Net-(K4-Pad5)")
    (add_net "Net-(K5-Pad1)")
    (add_net "Net-(K5-Pad2)")
    (add_net "Net-(K5-Pad3)")
    (add_net "Net-(K5-Pad4)")
    (add_net "Net-(K5-Pad5)")
    (add_net "Net-(K6-Pad1)")
    (add_net "Net-(K6-Pad2)")
    (add_net "Net-(K6-Pad3)")
    (add_net "Net-(K6-Pad4)")
    (add_net "Net-(K6-Pad5)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net OWC_BUS)
  )

  (net_class Power ""
    (clearance 1.5)
    (trace_width 3.75)
    (via_dia 2.5)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 120VAC)
    (add_net Compressor_Power)
  )

  (module TerminalBlock:TerminalBlock_Altech_AK300-2_P5.00mm (layer F.Cu) (tedit 59FF0306) (tstamp 63F14904)
    (at 43.18 86.36 180)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (path /63D7F975)
    (fp_text reference J1 (at -1.92 -6.99 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Screw_Terminal_01x02 (at 2.78 7.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 -2 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.65 -6.3) (end -2.65 6.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.65 6.3) (end 7.7 6.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.7 6.3) (end 7.7 5.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.7 5.35) (end 8.2 5.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.2 5.6) (end 8.2 3.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.2 3.7) (end 8.2 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.2 3.65) (end 7.7 3.9) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.7 3.9) (end 7.7 -1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.7 -1.5) (end 8.2 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.2 -1.2) (end 8.2 -6.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.2 -6.3) (end -2.65 -6.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.26 2.54) (end 1.28 2.54) (layer F.Fab) (width 0.1))
    (fp_line (start 1.28 2.54) (end 1.28 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.26 -0.25) (end 1.28 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.26 2.54) (end -1.26 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.74 2.54) (end 6.28 2.54) (layer F.Fab) (width 0.1))
    (fp_line (start 6.28 2.54) (end 6.28 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.74 -0.25) (end 6.28 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.74 2.54) (end 3.74 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -6.22) (end 7.61 -3.17) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -6.22) (end -2.58 -6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -6.22) (end 8.11 -6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 8.11 -6.22) (end 8.11 -1.4) (layer F.Fab) (width 0.1))
    (fp_line (start 8.11 -1.4) (end 7.61 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start 8.11 5.46) (end 7.61 5.21) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 5.21) (end 7.61 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 8.11 3.81) (end 7.61 4.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 4.06) (end 7.61 5.21) (layer F.Fab) (width 0.1))
    (fp_line (start 8.11 3.81) (end 8.11 5.46) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 6.22) (end 2.98 4.32) (layer F.Fab) (width 0.1))
    (fp_line (start 7.05 -0.25) (end 7.05 4.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 6.22) (end 7.05 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 7.05 6.22) (end 7.61 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 6.22) (end 2.04 4.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 6.22) (end 2.98 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start -2.02 -0.25) (end -2.02 4.32) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 6.22) (end -2.02 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start -2.02 6.22) (end 2.04 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 4.32) (end 7.05 4.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 4.32) (end 2.98 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 7.05 4.32) (end 7.05 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 4.32) (end -2.02 4.32) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 4.32) (end 2.04 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.02 4.32) (end -2.02 6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 6.67 3.68) (end 6.67 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.67 3.68) (end 3.36 3.68) (layer F.Fab) (width 0.1))
    (fp_line (start 3.36 3.68) (end 3.36 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start 1.66 3.68) (end 1.66 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start 1.66 3.68) (end -1.64 3.68) (layer F.Fab) (width 0.1))
    (fp_line (start -1.64 3.68) (end -1.64 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start -1.64 0.51) (end -1.26 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start 1.66 0.51) (end 1.28 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start 3.36 0.51) (end 3.74 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start 6.67 0.51) (end 6.28 0.51) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 6.22) (end -2.58 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 -0.64) (end -2.58 -3.17) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -1.65) (end 7.61 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -0.64) (end 7.61 4.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 -3.17) (end 7.61 -3.17) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 -3.17) (end -2.58 -6.22) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -3.17) (end 7.61 -1.65) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 -3.43) (end 2.98 -5.97) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 -5.97) (end 7.05 -5.97) (layer F.Fab) (width 0.1))
    (fp_line (start 7.05 -5.97) (end 7.05 -3.43) (layer F.Fab) (width 0.1))
    (fp_line (start 7.05 -3.43) (end 2.98 -3.43) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 -3.43) (end 2.04 -5.97) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 -3.43) (end -2.02 -3.43) (layer F.Fab) (width 0.1))
    (fp_line (start -2.02 -3.43) (end -2.02 -5.97) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 -5.97) (end -2.02 -5.97) (layer F.Fab) (width 0.1))
    (fp_line (start 3.39 -4.45) (end 6.44 -5.08) (layer F.Fab) (width 0.1))
    (fp_line (start 3.52 -4.32) (end 6.56 -4.95) (layer F.Fab) (width 0.1))
    (fp_line (start -1.62 -4.45) (end 1.44 -5.08) (layer F.Fab) (width 0.1))
    (fp_line (start -1.49 -4.32) (end 1.56 -4.95) (layer F.Fab) (width 0.1))
    (fp_line (start -2.02 -0.25) (end -1.64 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 2.04 -0.25) (end 1.66 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.66 -0.25) (end -1.64 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 -0.64) (end -1.64 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start -1.64 -0.64) (end 1.66 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start 1.66 -0.64) (end 3.36 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start 7.61 -0.64) (end 6.67 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start 6.67 -0.64) (end 3.36 -0.64) (layer F.Fab) (width 0.1))
    (fp_line (start 7.05 -0.25) (end 6.67 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 2.98 -0.25) (end 3.36 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 3.36 -0.25) (end 6.67 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.83 -6.47) (end 8.36 -6.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.83 -6.47) (end -2.83 6.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.36 6.47) (end 8.36 -6.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.36 6.47) (end -2.83 6.47) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 6.03 -4.59) (end 6.54 -5.05) (angle 90.5) (layer F.Fab) (width 0.1))
    (fp_arc (start 5.07 -6.07) (end 6.53 -4.12) (angle 75.5) (layer F.Fab) (width 0.1))
    (fp_arc (start 4.99 -3.71) (end 3.39 -5) (angle 100) (layer F.Fab) (width 0.1))
    (fp_arc (start 3.87 -4.65) (end 3.58 -4.13) (angle 104.2) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.03 -4.59) (end 1.53 -5.05) (angle 90.5) (layer F.Fab) (width 0.1))
    (fp_arc (start 0.06 -6.07) (end 1.53 -4.12) (angle 75.5) (layer F.Fab) (width 0.1))
    (fp_arc (start -0.01 -3.71) (end -1.62 -5) (angle 100) (layer F.Fab) (width 0.1))
    (fp_arc (start -1.13 -4.65) (end -1.42 -4.13) (angle 104.2) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 5 120VAC))
    (pad 2 thru_hole oval (at 5 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 Compressor_Power))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "Wemos D1 Mini:D1_mini_board" (layer F.Cu) (tedit 5766F65E) (tstamp 63E45819)
    (at 102.87 104.14)
    (path /63D7C335)
    (fp_text reference U1 (at 1.27 18.81) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value WeMos_mini (at 1.27 -19.05) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 11.431517 13.476932) (end 10.814156 13.476932) (layer F.SilkS) (width 0.1))
    (fp_line (start 11.431517 11.483738) (end 11.431517 13.476932) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.778878 11.483738) (end 11.431517 11.483738) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.796517 15.487765) (end 10.7436 9.402349) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.226656 15.487765) (end 10.796517 15.487765) (layer F.SilkS) (width 0.1))
    (fp_line (start 8.697489 14.993876) (end 9.226656 15.487765) (layer F.SilkS) (width 0.1))
    (fp_line (start 7.40985 14.993876) (end 8.697489 14.993876) (layer F.SilkS) (width 0.1))
    (fp_line (start 7.40985 9.931515) (end 7.40985 14.993876) (layer F.SilkS) (width 0.1))
    (fp_line (start 8.662211 9.931515) (end 7.40985 9.931515) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.191378 9.402349) (end 8.662211 9.931515) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.7436 9.402349) (end 9.191378 9.402349) (layer F.SilkS) (width 0.1))
    (fp_line (start -3.17965 15.865188) (end -3.17965 10.051451) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.959931 15.865188) (end -3.17965 15.865188) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.959931 10.051451) (end 3.959931 15.865188) (layer F.SilkS) (width 0.1))
    (fp_line (start -3.17965 10.051451) (end 3.959931 10.051451) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.83248 9.424181) (end 10.802686 16.232524) (layer F.SilkS) (width 0.1))
    (fp_line (start 12.776026 8.463285) (end 10.83248 9.424181) (layer F.SilkS) (width 0.1))
    (fp_line (start 12.751078 -14.091807) (end 12.776026 8.463285) (layer F.SilkS) (width 0.1))
    (fp_line (start 12.635482 -14.984575) (end 12.751078 -14.091807) (layer F.SilkS) (width 0.1))
    (fp_line (start 12.407122 -15.739613) (end 12.635482 -14.984575) (layer F.SilkS) (width 0.1))
    (fp_line (start 12.079595 -16.37146) (end 12.407122 -15.739613) (layer F.SilkS) (width 0.1))
    (fp_line (start 11.666503 -16.894658) (end 12.079595 -16.37146) (layer F.SilkS) (width 0.1))
    (fp_line (start 11.181445 -17.323743) (end 11.666503 -16.894658) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.638018 -17.673258) (end 11.181445 -17.323743) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.049824 -17.957741) (end 10.638018 -17.673258) (layer F.SilkS) (width 0.1))
    (fp_line (start 9.43046 -18.191734) (end 10.049824 -17.957741) (layer F.SilkS) (width 0.1))
    (fp_line (start -9.607453 -18.162976) (end 9.43046 -18.191734) (layer F.SilkS) (width 0.1))
    (fp_line (start -10.20525 -17.97731) (end -9.607453 -18.162976) (layer F.SilkS) (width 0.1))
    (fp_line (start -10.74944 -17.730377) (end -10.20525 -17.97731) (layer F.SilkS) (width 0.1))
    (fp_line (start -11.240512 -17.422741) (end -10.74944 -17.730377) (layer F.SilkS) (width 0.1))
    (fp_line (start -11.678953 -17.054952) (end -11.240512 -17.422741) (layer F.SilkS) (width 0.1))
    (fp_line (start -12.065253 -16.627577) (end -11.678953 -17.054952) (layer F.SilkS) (width 0.1))
    (fp_line (start -12.399901 -16.141167) (end -12.065253 -16.627577) (layer F.SilkS) (width 0.1))
    (fp_line (start -12.683384 -15.596286) (end -12.399901 -16.141167) (layer F.SilkS) (width 0.1))
    (fp_line (start -12.916195 -14.993493) (end -12.683384 -15.596286) (layer F.SilkS) (width 0.1))
    (fp_line (start -12.930193 16.176658) (end -12.916195 -14.993493) (layer F.SilkS) (width 0.1))
    (fp_line (start -3.849397 16.202736) (end -12.930193 16.176658) (layer F.SilkS) (width 0.1))
    (fp_line (start -3.851373 15.000483) (end -3.849397 16.202736) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.979849 14.993795) (end -3.851373 15.000483) (layer F.SilkS) (width 0.1))
    (fp_line (start 5.00618 16.277228) (end 4.979849 14.993795) (layer F.SilkS) (width 0.1))
    (fp_line (start 10.817472 16.277228) (end 5.00618 16.277228) (layer F.SilkS) (width 0.1))
    (fp_line (start -8.89 -17.78) (end -8.89 5.08) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 -17.78) (end -8.89 -17.78) (layer B.SilkS) (width 0.15))
    (fp_line (start 8.89 5.08) (end 8.89 -17.78) (layer B.SilkS) (width 0.15))
    (fp_line (start -8.89 5.08) (end 8.89 5.08) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.35 3.81) (end -6.35 3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start 6.35 -10.16) (end 6.35 3.81) (layer B.SilkS) (width 0.15))
    (fp_line (start -6.35 -10.16) (end 6.35 -10.16) (layer B.SilkS) (width 0.15))
    (fp_line (start -6.35 3.81) (end -6.35 -10.16) (layer B.SilkS) (width 0.15))
    (fp_text user WeMos (at 0 -15.24) (layer F.SilkS)
      (effects (font (size 3 3) (thickness 0.15)))
    )
    (pad 9 thru_hole circle (at 11.43 -10.16) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 -7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 11.43 -5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 11.43 -2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 11.43 0) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 11.43 2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 11.43 5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at 11.43 7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad16)"))
    (pad 1 thru_hole circle (at -11.43 7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 5VDC))
    (pad 2 thru_hole circle (at -11.43 5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 Gnd))
    (pad 3 thru_hole circle (at -11.43 2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 0) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 Compressor_Signal))
    (pad 5 thru_hole circle (at -11.43 -2.54) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 OWC_BUS))
    (pad 6 thru_hole circle (at -11.43 -5.08) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at -11.43 -7.62) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at -11.43 -10.16) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad8)"))
  )

  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148) (tstamp 63E45189)
    (at 201.93 88.5)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (path /63D7C91B)
    (fp_text reference K6 (at 8.1 9.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.05 1.85) (end 4.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 -1.75) (end 8.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 8.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 1.85) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 6.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 9.45 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 3.65) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.95 0.05) (end 15.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 10.95 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 3.55 -5.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 1.85 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.55 6.05) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 -4.2) (end 14.15 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 4.2) (end 14.15 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 7.7) (end -1.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 7.7) (end -1.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 -7.7) (end 18.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start -1.3 -7.7) (end 18.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 18.4 7.8) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 -7.8) (end 18.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end 18.4 -7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end -1.4 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 1.2) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(K6-Pad1)"))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(K6-Pad5)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(K6-Pad4)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 "Net-(K6-Pad3)"))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(K6-Pad2)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148) (tstamp 63E45160)
    (at 179.66 88.5)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (path /63D7C8F1)
    (fp_text reference K5 (at 8.1 9.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1.2) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end -1.4 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end 18.4 -7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 -7.8) (end 18.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 7.8) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -7.7) (end 18.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 -7.7) (end 18.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 7.7) (end -1.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start -1.3 7.7) (end -1.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 18.55 -7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.15 4.2) (end 14.15 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 -4.2) (end 14.15 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.55 6.05) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 1.85 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 3.55 -5.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 10.95 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.95 0.05) (end 15.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 3.65) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 9.45 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 6.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 1.85) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 8.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 -1.75) (end 8.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 1.85) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(K5-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(K5-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(K5-Pad4)"))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(K5-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(K5-Pad1)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148) (tstamp 63E45137)
    (at 157.25 88.55)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (path /63D7C85B)
    (fp_text reference K4 (at 8.1 9.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.05 1.85) (end 4.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 -1.75) (end 8.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 8.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 1.85) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 6.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 9.45 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 3.65) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.95 0.05) (end 15.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 10.95 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 3.55 -5.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 1.85 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.55 6.05) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 -4.2) (end 14.15 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 4.2) (end 14.15 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 7.7) (end -1.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 7.7) (end -1.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 -7.7) (end 18.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start -1.3 -7.7) (end 18.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 18.4 7.8) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 -7.8) (end 18.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end 18.4 -7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end -1.4 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 1.2) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(K4-Pad1)"))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(K4-Pad5)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(K4-Pad4)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(K4-Pad3)"))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(K4-Pad2)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148) (tstamp 63E4510E)
    (at 134.62 88.55)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (path /63D7C745)
    (fp_text reference K3 (at 8.1 9.2) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1.2) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end -1.4 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end 18.4 -7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 -7.8) (end 18.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 7.8) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -7.7) (end 18.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 -7.7) (end 18.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 7.7) (end -1.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start -1.3 7.7) (end -1.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 18.55 -7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.15 4.2) (end 14.15 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 -4.2) (end 14.15 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.55 6.05) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 1.85 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 3.55 -5.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 10.95 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.95 0.05) (end 15.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 3.65) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 9.45 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 6.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 1.85) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 8.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 -1.75) (end 8.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 1.85) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(K3-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(K3-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(K3-Pad4)"))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(K3-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(K3-Pad1)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148) (tstamp 63E450E5)
    (at 43.48 142.42 90)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (path /63D7CA49)
    (fp_text reference K2 (at 8.1 9.2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 8.05 1.85) (end 4.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 -1.75) (end 8.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 8.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 1.85) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 6.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 9.45 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 3.65) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.95 0.05) (end 15.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 10.95 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 3.55 -5.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 1.85 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.55 6.05) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 -4.2) (end 14.15 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 4.2) (end 14.15 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 7.1 0.025 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 7.7) (end -1.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 7.7) (end -1.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 -7.7) (end 18.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start -1.3 -7.7) (end 18.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_text user 1 (at 0 -2.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 18.4 7.8) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 -7.8) (end 18.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end 18.4 -7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end -1.4 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 1.2) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 120VAC))
    (pad 5 thru_hole circle (at 1.95 -5.95 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 Compressor_Signal))
    (pad 4 thru_hole circle (at 14.2 -6 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 Compressor_Power))
    (pad 3 thru_hole circle (at 14.15 6.05 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(K2-Pad3)"))
    (pad 2 thru_hole circle (at 1.95 6.05 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 Gnd))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148) (tstamp 63E450BC)
    (at 43.485001 118.11 90)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (path /63D7CA77)
    (fp_text reference K1 (at 8.1 9.2 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 1.2) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end -1.4 -1.2) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 -7.8) (end 18.4 -7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 -7.8) (end 18.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 18.4 7.8) (end -1.4 7.8) (layer F.SilkS) (width 0.12))
    (fp_text user 1 (at 0 -2.3 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -7.7) (end 18.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 -7.7) (end 18.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start 18.3 7.7) (end -1.3 7.7) (layer F.Fab) (width 0.12))
    (fp_line (start -1.3 7.7) (end -1.3 -7.7) (layer F.Fab) (width 0.12))
    (fp_text user %R (at 7.1 0.025 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 18.55 -7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end -1.55 -7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 18.55 -7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 7.95) (end 18.55 7.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.15 4.2) (end 14.15 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 14.15 -4.2) (end 14.15 -1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.55 6.05) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 1.85 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 3.55 -5.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 10.95 0.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.95 0.05) (end 15.55 -2.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 3.65) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.45 0.05) (end 9.45 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.65 0.05) (end 2.65 3.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 -5.95) (end 6.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.05 1.85) (end 6.05 6.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 1.85) (end 4.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 8.05 -1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 -1.75) (end 8.05 1.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.05 1.85) (end 4.05 1.85) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 1.95 6.05 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 Gnd))
    (pad 3 thru_hole circle (at 14.15 6.05 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(K1-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 Compressor_Power))
    (pad 5 thru_hole circle (at 1.95 -5.95 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 Compressor_Signal))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 120VAC))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 56.475001 109.22) (end 49.535001 116.16) (width 1) (layer F.Cu) (net 1))
  (segment (start 91.44 109.22) (end 56.475001 109.22) (width 1) (layer F.Cu) (net 1))
  (segment (start 38.18 103.215001) (end 37.485001 103.91) (width 3.75) (layer F.Cu) (net 3))
  (segment (start 38.18 86.36) (end 38.18 103.215001) (width 3.75) (layer F.Cu) (net 3))
  (segment (start 35.980001 126.720001) (end 37.48 128.22) (width 3.75) (layer F.Cu) (net 3))
  (segment (start 32.91 123.65) (end 35.980001 126.720001) (width 3.75) (layer F.Cu) (net 3))
  (segment (start 32.91 108.485001) (end 32.91 123.65) (width 3.75) (layer F.Cu) (net 3))
  (segment (start 37.485001 103.91) (end 32.91 108.485001) (width 3.75) (layer F.Cu) (net 3))
  (segment (start 36.280001 139.220001) (end 37.53 140.47) (width 1) (layer B.Cu) (net 4))
  (segment (start 33.979999 136.919999) (end 36.280001 139.220001) (width 1) (layer B.Cu) (net 4))
  (segment (start 37.535001 117.927766) (end 33.979999 121.482768) (width 1) (layer B.Cu) (net 4))
  (segment (start 33.979999 121.482768) (end 33.979999 136.919999) (width 1) (layer B.Cu) (net 4))
  (segment (start 37.535001 116.16) (end 37.535001 117.927766) (width 1) (layer B.Cu) (net 4))
  (segment (start 37.535001 116.16) (end 44.475001 109.22) (width 1) (layer B.Cu) (net 4))
  (segment (start 44.475001 109.22) (end 81.28 109.22) (width 1) (layer B.Cu) (net 4))
  (segment (start 86.36 104.14) (end 91.44 104.14) (width 1) (layer B.Cu) (net 4))
  (segment (start 81.28 109.22) (end 86.36 104.14) (width 1) (layer B.Cu) (net 4))
  (segment (start 43.18 117.804999) (end 43.485001 118.11) (width 3.75) (layer F.Cu) (net 5))
  (segment (start 43.18 86.36) (end 43.18 117.804999) (width 3.75) (layer F.Cu) (net 5))
  (segment (start 43.485001 142.414999) (end 43.48 142.42) (width 3.75) (layer F.Cu) (net 5))
  (segment (start 43.485001 118.11) (end 43.485001 142.414999) (width 3.75) (layer F.Cu) (net 5))

)
