# Beer Gravity Monitor

...
A sleep-interval of less than 300s will reduce battery life, consider using 900s
When using the gyro temperature use a sleep-interval that is greater than 300s for accurate readings

##

Device name:
Temperature Format:
Celsius
Farenheight
Interval (seconds):

Current calibration values: Loading... Loading...

##

Http URL 1:
Http URL 2:

Brewfather URL:

InfluxDB v2 URL:
InfluxDB v2 Org:
InfluxDB v2 Bucket:
InfluxDB v2 Auth:

MQTT Server:
MQTT Port:
MQTT User:
MQTT Password:

##

Gravity Format:
SG
Plato
Formula (SG)
Temperature adjust gravity

##

Voltage factor:
Loading...
Temp Sensor Adj:
Use gyro temperature
OTA base URL:

##### Define HTTP headers

Header 1 (Header: value) Header 2 (Header: value)
(C) Copyright 2021-22 Magnus Persson