# Compiling the software - GravityMon 0.9.0 documentation

Hide navigation sidebar
Hide table of contents sidebar
Back to top
Toggle table of contents sidebar

# Compiling the software

## Tools

I use the following tools in order to build and manage the software:

- Visual Studio Code

- PlatformIO

- Git for Windows

- VSCode plugin: Minify (used to minimise the html files)

## Code Formatting

I use pre-commit and their cpp style checks to validate the code. Plugin defintions are found in .pre-commit-config.yaml

Pre-Commit

Note

There is not yet any automatic checks since this does not work on Windows. It works if running under WSL2 with Ubuntu.

## Targets

In the platformio config there are 3 targets defined

- gravity-debug; Maximum logging for trouble shooting, deep sleep is disabled.

- gravity-release; Standard release

- gravity-perf; Standard release but contains code for measuring performance

- gravity32-perf: Experimental version for ESP32.

Note

There is an experimental ESP32 target but since platformio only supports SDK 1.0.6 and the WIFI connection is really slow compared to ESP8266, so the recommendation is to wait for support on 2.0.x branch. With the tested version an wifi connection takes 3-8s on a ESP32 compared to 0.5s on an ESP8266. There is also a bug in OneWire connected to ESP32 that has not been fixed in the main repository yet.

Warning

The debug target can be unstable and crash the device under certain circumstanses. Excessive logging to the serial port can cause corruption and crashes. So only enable enough debugging to troubleshoot your changes.

## Source structure

Directory structure
path | content
--- | ---
/bin | Contains compiled binaries
/data | Directory for flashing device filesystem
/doc | Various external documents used as input
/html | Source for html files
/img | Images uses in README.md
/lib | External libraries used when compiling
/script | Scripts used in build process
/src | Source code for software
/src_docs | Source code for documentation
/stl | 3d models
/test | Test data for developing html files

## Options

This is a list of C++ defines that is used to enable/disable functions in the code.

Defines
define | description
--- | ---
ACTIVATE_OTA | Enables the OTA functionallity in the code
SKIP_SLEEPMODE | The device never goes into sleep mode, useful when developing.
xxx_DISABLE_LOGGING | Done include verbose logging in the corresponding class. Excessive logging may crash device.
USE_LITTLEFS | Use the new filesystem in Ardurino
EMBED_HTML | Html files are included in code, if not defined they are served from the file system.
USER_SSID | If defined the device will always use this SSID
USER_SSID_PWD | Password to the SSID
CFG_APPVER | Defines the version of the compiled software